
Lonzone Topping Compound 
Product Data Sheet
[bookmark: heading_0]Product Description
Lonzone Topping Compound is a premium quality, pre-mixed, semi-lightweight topping compound designed for exceptional flow and workability. It delivers a smooth, even finish with excellent sandability and paintability, making it ideal for professional drywall finishing applications.
This ready-to-use finishing compound is formulated to provide superior coverage and a creamy consistency that allows for easy application and feathering. Lonzone Topping Compound is specifically engineered for the final coat in a three-coat drywall jointing system.
[bookmark: heading_1]Recommended Use
Lonzone Topping Compound is used as a top coat in a three-coat drywall jointing system, suitable for finishing gypsum board and fibre cement joints, internal angles, and fastener heads in residential and commercial walls and ceilings.
While Lonzone Topping Compound can be hand applied, it has exceptional flow when applied through a finishing box for maximum efficiency. For optimal results, it is recommended that Lonzone Topping Compound be used in conjunction with Lonzone Base Coat or All-Purpose Joint Compounds.
[bookmark: heading_2]Important Notes
· Do not use for bedding tape or laminating drywall sheets
· In wet area applications, topping compounds should not be used on areas to be tiled
· Lonzone Topping Compound can be thinned sparingly with clean water if required
· Do not apply setting-type compounds over Lonzone Topping Compound
· Should not be used when the interior lining temperature is less than 8°C
· Ensure surfaces are clean from dust, dirt, or grease
· Before use, remix to a smooth creamy consistency
· Always use clean containers and equipment
· Thoroughly clean tools immediately after use
· Replace lid tightly when not in use
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Store pails of compound in a dry environment out of direct sunlight. Protect from freezing. Remove lid and stir thoroughly prior to use. Unused product should be stored by resealing the original pail. Remix prior to use. Discard if drying has commenced or if product shows signs of spoilage.
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· Exceptional Flow — Ideal for both hand and machine application
· Pre-mixed & Ready to Use — Smooth consistency is quick to prepare and easy to apply
· Grit Free Formula — Delivers a perfectly smooth finish with excellent sandability
· Superior Paintability — Provides an excellent base for paint application
· Low Shrinkage — Minimizes cracking and requires less sanding
· Low VOC — Meets strict environmental standards
[bookmark: heading_5]Product Specifications
	Feature
	Description

	Colour
	Off White

	Coverage
	[bookmark: _GoBack]Approximately 9-11 kg per 100 m² (for joint finishing)

	Packaging
	15 kg Re-sealable pail

	Shelf Life
	12 months from date of manufacture

	Specific Gravity
	1.2 - 1.6

	VOC Content
	Less than 1 g/L

	Drying Time
	Approximately 24 hours at 20°C and 50% RH

	Application Temperature
	Minimum 8°C 


[bookmark: heading_6]Application Instructions
[bookmark: heading_7]Hand Application
1、Allow adequate time for the second coat to harden completely before applying the Lonzone Topping Compound final coat.
2、Using a 250mm or 300mm broadknife, apply a thin topping coat wide enough to conceal the previously coated joint. Feather the edges of the compound with a trowel for a seamless finish.
3、Using a 100mm broadknife, cover previously coated fastener heads, overlapping about 25mm beyond the fastener area.
4、For internal angles, apply compound to both sides of the corner using a corner trowel.
[bookmark: heading_8]Machine Application
Apply a thin topping coat of Lonzone Topping Compound using a 250mm or 300mm finishing box. Adjust box pressure to achieve a uniform thin coat. For best results, maintain consistent speed and pressure during application.
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Allow Lonzone Topping Compound to dry for at least 24 hours before sanding. Sand to a smooth finish using 180 grit sandpaper or 180-220 grit sanding mesh. For professional results, use a pole sander with gentle, even pressure. Always wear appropriate respiratory protection during sanding operations.
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Apply all paints in accordance with the paint manufacturer recommendations. Ensure the surface is completely dry, clean, and free of dust before applying primer or paint. Lonzone Topping Compound provides an excellent base for all types of interior paints.
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Lonzone Topping Compound meets or exceeds the requirements of applicable industry standards for drywall finishing compounds. For specific certification details or test reports, please contact our technical support team.
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Refer to the Safety Data Sheet (SDS) for this product for detailed health and safety information. Always use appropriate personal protective equipment (PPE) including eye protection and gloves. Ensure adequate ventilation during application and sanding. Avoid contact with eyes and prolonged skin contact. Keep out of reach of children.
For SDS requests or health and safety inquiries, contact:
Lonzone Technical Department
Email:  
Phone:  
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For further information on this product or for technical support, please contact our customer service team:
LONZONE Environmental Protection (Suzhou) Co., Ltd 
Website: 
Email: 
Customer Service: 
	For optimal performance, use Lonzone Topping Compound as part of a complete Lonzone drywall finishing system, including Lonzone Base Coat Compound and Lonzone Joint Tape.




